Head office VDI endpoint refresh
Thin client selection and design
	Customer
	Niyyasoft

	Site
	Riyadh HQ

	Prepared by
	Niyyasoft

	Date
	30 September 2026

	Recommendation
	263 x Dell Pro Micro Thin Client (Q9M1260) · 100% fit · meets every requirement



Prepared with the Zero/Thin Client Selector by Niyya Software. Specifications are taken from each OEM's official website.
1. Executive summary
For 250 knowledge worker seats on Citrix, the tool scored 233 current models from 29 OEMs against 2 x Full HD displays, a 1 GbE network, optimised Microsoft Teams and the ports, peripherals, management and security asked for. The recommended endpoint is the Dell Pro Micro Thin Client (Q9M1260) from Dell Technologies, running Dell ThinOS 10.x, at 100% fit. It meets every stated requirement on the OEM's published data. 263 endpoints are needed (250 seats plus 13 spares). 22 of the 233 models meet every requirement and 64 more need a value confirming.
	Endpoints
	263 (250 seats + 13 spares)

	Device
	Dell Pro Micro Thin Client (Q9M1260) - Thin client · Desktop box

	Operating system
	Dell ThinOS 10.x

	Fit
	100% - meets every requirement

	Platform and protocol
	Citrix over Citrix HDX (ICA)

	Processor and memory
	Intel Processor N150 (4 cores, up to 3.6 GHz); Intel Processor N250 (4 cores, up to 3.8 GHz); Intel Core 3 Processor N350 (8 cores, up to 3.9 GHz) · 8 - 16 GB DDR5 SO-DIMM (1 module, 4800 MT/s)

	Displays
	5 displays, up to 3840x2160@60 · 2 x DisplayPort, 1 x USB-C (DP Alt)

	USB and network
	3 x USB 2.0, 1 x USB 3.x, 2 x USB-C · 1 GbE, Wi-Fi 7

	VDI platforms
	Citrix, Omnissa Horizon, Azure Virtual Desktop, Windows 365, Microsoft RDS, Amazon WorkSpaces, HP Anyware, Parallels RAS, Frame, Workspot, Leostream

	Optimised UC
	Microsoft Teams, Zoom, Cisco Webex, Cisco Jabber, Skype for Business

	Management
	Wyse Management Suite

	Official source
	https://www.dell.com/en-us/shop/wyse-endpoints-and-software/dell-pro-micro-thin-client/spd/dell-pro-q9m1260-thin-client-micro



2. Requirements
	Item
	Requirement

	Use case
	Knowledge worker - 250 users, 5% spares, 80% signed in at peak

	VDI platform
	Citrix DaaS / Virtual Apps and Desktops - virtual desktops (VDI)

	Display protocol
	Citrix HDX (ICA) (the platform's own)

	Device
	Type: thin or zero client; form factor: desktop box; operating system: any

	Displays
	2 x Full HD (1920 x 1080) per seat; preferred port: any

	Processor, memory, storage
	At least 4 cores, 8 GB memory, 16 GB storage (the tool's baseline for this use case)

	Network
	1 GbE wired; Wired only; Office, on the campus LAN

	Connectivity options
	None

	USB and ports
	At least 4 USB ports

	Unified communications
	Microsoft Teams - optimised on the endpoint

	Peripherals
	Webcam, Headset, Printer

	Management and security
	Central management software, TPM 2.0

	OEMs considered
	All (35)



3. How it was worked out
	Step
	Working

	Seats
	250 users + 5% spares (13) = 263 endpoints to buy

	Per-seat baseline
	Knowledge worker baseline: 4 cores, 8 GB. A planning rule of thumb, not an OEM figure.

	Per-seat minimum used
	4 cores, 8 GB memory, 16 GB storage

	Displays
	2 x Full HD per seat = 500 screens in total

	USB at the desk
	4 devices: Keyboard, Mouse, Webcam, Headset

	Session bandwidth
	0.9 Mbps average per session (knowledge worker, 2 displays at Full HD) x 200 concurrent users (80%) + 50 in calls at 1.5 Mbps = about 255 Mbps on the site uplink. A planning estimate - measure a pilot before sizing the WAN.

	Access network
	250 wired ports at 1 GbE; 6 x 48-port access switches with 10% spare ports



Every model is scored 0-100 on each criterion that applies and the scores are weighted into the fit percentage. A hard mismatch - wrong device type, platform not supported, too few displays, no Wi-Fi when Wi-Fi is the link - caps the fit at 49%. A value the OEM does not publish is listed as "to confirm" and scored low.
4. Recommended device
Dell Pro Micro Thin Client (Q9M1260)
Thin client · Desktop box · Dell ThinOS 10.x
Dell's current fanless micro thin client with up to an 8-core Intel N-series CPU, a swappable rear expansion module (fibre, second NIC, serial, extra video) and support for up to five displays.
Fit breakdown
	Criterion
	Weight
	Score

	VDI platform & protocol
	20
	100%

	Device type & OS
	9
	100%

	Displays
	14
	100%

	CPU, memory & storage
	13
	100%

	Network & connectivity
	10
	100%

	USB & ports
	7
	100%

	Teams / UC, camera & audio
	10
	100%

	Peripherals
	5
	100%

	Management & security
	6
	100%

	Use-case suitability
	4
	100%

	Model currency
	2
	100%



Bill of materials
	Item
	Specification
	Quantity

	Endpoint
	Dell Pro Micro Thin Client (Q9M1260) (Thin client · Desktop box) - 250 seats + 13 spares
	263

	Operating system
	Dell ThinOS 10.x
	263

	Memory
	8 GB DDR5 SO-DIMM (1 module, 4800 MT/s)
	263

	Storage
	At least 16 GB - 128 GB UFS (M.2 2230) or 256 GB M.2 2230 PCIe NVMe SSD
	263

	Monitor
	Full HD (1920 x 1080) monitor, 2 per seat
	500

	Video cable
	To match the device outputs: 2 x DisplayPort, 1 x USB-C (DP Alt)
	500

	Keyboard and mouse
	USB keyboard and mouse set
	250

	Webcam
	USB webcam (UVC), Full HD
	250

	Headset
	Microsoft Teams-certified headset, USB or 3.5 mm
	250

	Management software
	Wyse Management Suite - one managed device each
	263

	VDI client
	Citrix Workspace app for Citrix, as included with or installed on Dell ThinOS 10.x
	263

	Access switch port
	1 GbE port and patch cable
	250



5. Logical design
[image: ]
Figure 1 - Logical design. Users, the endpoint and its peripherals, the network, gateway and broker, desktops and apps, with management, collaboration and security.
6. Implementation design
[image: ]
Figure 2 - Implementation design. Seat wiring by port, the network path from desk to desktop, quantities and rollout.
Port plan per seat
	Connects
	Port on the device

	Monitor 1
	DisplayPort 1

	Monitor 2
	DisplayPort 2

	Keyboard
	USB 2.0 1

	Mouse
	USB 2.0 2

	Webcam
	USB 3.x 1

	Headset
	3.5 mm audio jack (or USB)

	Printer
	Network printer, or a spare USB port

	Network
	RJ-45 1 GbE to the access switch

	Power
	65 W adapter



Quantities
	Item
	Quantity

	Endpoints for seats
	250

	Spares (5%)
	13

	Endpoints to buy
	263

	Monitors
	500 (2 per seat)

	Access switch ports
	250 at 1 GbE

	48-port access switches
	6

	Managed devices
	263 in Wyse Management Suite

	Site uplink at peak
	about 255 Mbps

	Power adapters, rated
	16.3 kW across the seats



Rollout
1. Stand up Wyse Management Suite and enrol one test device (DHCP option or DNS record for auto-discovery).
2. Build the device profile: Dell ThinOS 10.x, Citrix Workspace app, 2-display layout, Microsoft Teams optimisation, peripheral and USB policy.
3. Prepare the network: endpoint VLAN and DHCP scope for 263 devices, 1 GbE access ports, QoS for real-time media, firewall rules (TCP/UDP 443 through the gateway; 1494 / 2598 on the LAN).
4. Pilot 10 seats across the knowledge worker use case; measure session bandwidth against the 0.9 Mbps per-session estimate.
5. Roll out by floor or site: 250 seats, zero-touch enrolment, asset tags, user sign-off per batch.
6. Hand over: 13 spares on the shelf, firmware and OS update cadence, OEM support contacts.
7. Alternatives from other OEMs
The best-fitting model from each OEM for the same requirements.
	OEM
	Model
	Type
	Fit
	Status
	To resolve

	Dell
	Dell Pro Micro Thin Client (Q9M1260)
	Thin client · Desktop box
	100%
	Meets
	-

	HP
	HP Elite t655 Thin Client
	Thin client · Desktop box
	100%
	Meets
	-

	Praim
	Meridian (M9354 / M9311 / M9321)
	Thin client · Desktop box
	99%
	Meets
	-

	10ZiG
	7300q Series (7372q / 7311q)
	Thin client · Desktop box
	98%
	Meets
	-

	Lenovo
	ThinkCentre M75q Gen 5
	Thin client · Desktop box
	97%
	Meets
	-

	LG
	CQ601 (CQ601N / CQ601I / CQ601W)
	Thin client · Desktop box
	97%
	Meets
	-

	Centerm
	D650
	Thin client · Desktop box
	97%
	To confirm
	Confirm: optimised Microsoft Teams on Windows IoT is inferred, not stated by the OEM

	ZeeTim
	ZeeTerm ZTX6002
	Thin client · Desktop box
	97%
	To confirm
	Confirm: tPM is not published

	NComputing
	EX500S
	Thin client · Desktop box
	96%
	To confirm
	Confirm: tPM is not published

	Rangee
	Rangee Thin Client RT-603
	Thin client · Desktop box
	96%
	To confirm
	Confirm: tPM is not published

	ClearCube
	CD8810
	Thin client · Desktop box
	96%
	To confirm
	Confirm: tPM is not published

	Atrust
	t175W
	Thin client · Desktop box
	96%
	To confirm
	Confirm: optimised Microsoft Teams on Windows IoT is inferred, not stated by the OEM

	Chip PC
	iX PC Core Wifi
	Thin client · Desktop box
	95%
	To confirm
	Confirm: optimised Microsoft Teams on Windows IoT is inferred, not stated by the OEM; Confirm: tPM is not published

	Leadtek
	EL4115 Ultra-Thin Client
	Thin client · Desktop box
	95%
	To confirm
	Confirm: optimised Microsoft Teams on Windows IoT is inferred, not stated by the OEM; Confirm: tPM is not published

	Fujitsu
	ESPRIMO G6016-TC
	Thin client · Desktop box
	95%
	To confirm
	Confirm: optimised Microsoft Teams on Windows IoT is inferred, not stated by the OEM; Confirm: no central management software is named by the OEM

	Amulet Hotkey
	DX1500
	Thin client · Desktop box
	94%
	To confirm
	Confirm: processor core count is not published

	OnLogic
	TM260
	Zero client · Desktop box
	91%
	To confirm
	Confirm: optimised Microsoft Teams support is not published; Confirm: tPM is not published

	Clientron
	G610
	Thin client · Desktop box
	90%
	To confirm
	Confirm: optimised Microsoft Teams on Windows IoT is inferred, not stated by the OEM; Confirm: no central management software is named by the OEM

	openthinclient
	ThinClient BLACK.QUADRO.II
	Thin client · Desktop box
	88%
	To confirm
	Confirm: wired Ethernet speed is not published; Confirm: optimised Microsoft Teams support is not published; Confirm: tPM is not published

	Pepperl+Fuchs
	BTC22
	Thin client · Desktop box
	84%
	Short
	1 USB port; 4 needed; Confirm: processor core count is not published; Confirm: tPM is not published

	epatec
	Thin Client 13G
	Thin client · Desktop box
	83%
	Short
	4 GB memory at most; 8 GB recommended for this use case; Confirm: maximum resolution is not published; Confirm: processor core count is not published; Confirm: no central management software is named by the OEM; Confirm: tPM is not published

	RDP
	RDP Thin Client C212261
	Thin client · Desktop box
	79%
	Short
	1 USB port; 4 needed; Confirm: maximum resolution is not published; Confirm: processor core count is not published; Confirm: optimised Microsoft Teams on Windows IoT is inferred, not stated by the OEM; Confirm: no central management software is named by the OEM; Confirm: tPM is not published

	Raspberry Pi
	Raspberry Pi 500
	Thin client · Desktop box
	77%
	Short
	3 USB ports; 4 needed; Confirm: vDI platform support is not published by the OEM; Confirm: optimised Microsoft Teams support is not published; Confirm: no central management software is named by the OEM; Confirm: tPM is not published

	Advantech
	TPC-312 EHL
	Thin client · All-in-one 12.1"
	49%
	Short
	Is all-in-one, not desktop box; Confirm: number of displays supported is not published; Confirm: maximum resolution is not published; Confirm: optimised Microsoft Teams on Windows IoT is inferred, not stated by the OEM

	Microsoft
	Windows 365 Link
	Thin client · Desktop box
	49%
	Short
	No Citrix support published (lists Windows 365); Confirm: processor core count is not published; Confirm: optimised Microsoft Teams support is not published

	Rockwell
	ASEM 6300T-BB Dual DisplayPort Thin Client
	Zero client · Desktop box
	49%
	Short
	No Citrix support published (lists Other); Confirm: optimised Microsoft Teams support is not published; Confirm: tPM is not published

	IGEL
	IGEL UD Pocket 2
	Thin client · Stick / board
	49%
	Short
	Is stick / board, not desktop box; 0 USB ports; 4 needed; No USB port for a webcam; No audio jack or USB port for a headset; No port for a printer; Confirm: number of displays supported is not published; Confirm: maximum resolution is not published; Confirm: processor core count is not published; Confirm: memory is not published; Confirm: wired Ethernet speed is not published; Confirm: tPM is not published

	vCloudPoint
	V1
	Zero client · Desktop box
	49%
	Short
	No Citrix support published (lists vCloudPoint vMatrix); Drives 1 display; 2 needed; Confirm: optimised Microsoft Teams support is not published; Confirm: tPM is not published

	Thinvent
	Thinvent Micro 6 Pro
	Thin client · Desktop box
	49%
	Short
	No Citrix support published (lists Microsoft RDP, Terminal emulation, Browser / HTML5); Drives 1 display; 2 needed; 4 GB memory at most; 8 GB recommended for this use case; 100 Mb Ethernet; 1 GbE needed; 2 USB ports; 4 needed; Confirm: maximum resolution is not published; Confirm: optimised Microsoft Teams support is not published; Confirm: tPM is not published



Top of the ranking
	#
	OEM
	Model
	Type
	Fit
	Status

	1
	Dell
	Dell Pro Micro Thin Client (Q9M1260)
	Thin client · Desktop box
	100%
	Meets

	2
	HP
	HP Elite t655 Thin Client
	Thin client · Desktop box
	99.8%
	Meets

	3
	HP
	HP Elite t660 Thin Client
	Thin client · Desktop box
	99.8%
	Meets

	4
	HP
	HP Pro t550 Thin Client
	Thin client · Desktop box
	99.8%
	Meets

	5
	HP
	HP ProDesk 5 G1i Thin Client
	Thin client · Desktop box
	99.8%
	Meets

	6
	Praim
	Meridian (M9354 / M9311 / M9321)
	Thin client · Desktop box
	99.2%
	Meets

	7
	10ZiG
	7300q Series (7372q / 7311q)
	Thin client · Desktop box
	98.4%
	Meets

	8
	10ZiG
	7000q Series (7072q / 7010q / 7011q)
	Thin client · Desktop box
	98.2%
	Meets

	9
	HP
	HP Elite t755 Thin Client
	Thin client · Desktop box
	98%
	Meets

	10
	Praim
	Neutrino (N9254 / N9211 / N9221)
	Thin client · Desktop box
	97.8%
	Meets

	11
	Lenovo
	ThinkCentre M75q Gen 5
	Thin client · Desktop box
	97.4%
	Meets

	12
	Lenovo
	ThinkCentre neo 50q Gen 5
	Thin client · Desktop box
	97.4%
	Meets

	13
	Lenovo
	ThinkCentre neo 55q Gen 6
	Thin client · Desktop box
	97.4%
	Meets

	14
	Lenovo
	ThinkEdge SE10n Gen2
	Thin client · Desktop box
	97.4%
	Meets

	15
	Lenovo
	ThinkEdge SE30n Gen2
	Thin client · Desktop box
	97.4%
	Meets

	16
	Praim
	Zenith (Z9354 / Z9311)
	Thin client · Desktop box
	97.4%
	Meets

	17
	Lenovo
	ThinkEdge SE10
	Thin client · Desktop box
	97.2%
	Meets

	18
	Lenovo
	ThinkCentre M70q Gen 5
	Thin client · Desktop box
	96.7%
	Meets

	19
	Lenovo
	ThinkCentre M70q Gen 6
	Thin client · Desktop box
	96.7%
	Meets

	20
	LG
	CQ601 (CQ601N / CQ601I / CQ601W)
	Thin client · Desktop box
	96.6%
	Meets



8. Model comparison
Recommended from the comparison: Dell Pro Micro Thin Client (Q9M1260) at 100% fit.
	
	Dell Pro Micro Thin Client (Q9M1260)
	HP Elite t655 Thin Client
	Praim Meridian (M9354 / M9311 / M9321)
	10ZiG 7300q Series (7372q / 7311q)
	Lenovo ThinkCentre M75q Gen 5

	Fit
	100%
	99.8%
	99.2%
	98.4%
	97.4%

	Status
	Meets
	Meets
	Meets
	Meets
	Meets

	VDI platform & protocol
	100%
	100%
	100%
	100%
	100%

	Device type & OS
	100%
	100%
	100%
	100%
	100%

	Displays
	100%
	100%
	100%
	100%
	100%

	CPU, memory & storage
	100%
	100%
	100%
	100%
	100%

	Network & connectivity
	100%
	100%
	100%
	100%
	100%

	USB & ports
	100%
	100%
	100%
	100%
	100%

	Teams / UC, camera & audio
	100%
	100%
	94%
	94%
	92%

	Peripherals
	100%
	100%
	100%
	80%
	80%

	Management & security
	100%
	100%
	100%
	100%
	100%

	Use-case suitability
	100%
	100%
	100%
	100%
	82%

	Model currency
	100%
	90%
	90%
	100%
	100%

	Type
	Thin client · Desktop box
	Thin client · Desktop box
	Thin client · Desktop box
	Thin client · Desktop box
	Thin client · Desktop box

	Operating systems
	Dell ThinOS, Windows IoT Enterprise
	Vendor Linux, Windows IoT Enterprise, IGEL OS
	Vendor Linux, Windows IoT Enterprise
	Vendor Linux, Windows IoT Enterprise
	IGEL OS, Windows IoT Enterprise

	Processor
	Intel Processor N150 (4 cores, up to 3.6 GHz); Intel Processor N250 (4 cores, up to 3.8 GHz); Intel Core 3 Processor N350 (8 cores, up to 3.9 GHz)
	AMD Ryzen Embedded R2314 (4 cores / 4 threads, 2.1 GHz base, up to 3.5 GHz)
	Intel N97 Quad-Core up to 3.6GHz (Alder Lake)
	Intel N100 Quad Core up to 3.40GHz
	AMD Ryzen 3 / 5 8000 or Ryzen 3 / 5 / 7 PRO 8000 Series, up to Ryzen 7 PRO 8700G / 8700GE

	Memory
	8 - 16 GB DDR5 SO-DIMM (1 module, 4800 MT/s)
	4 - 32 GB DDR4 SODIMM (dual channel, 2 slots, up to 2667 MT/s)
	8 - 16 GB
	8 - 16 GB
	64 GB DDR5-5200 SO-DIMM (two slots; 32GB standard maximum, 64GB by special bid)

	Displays / max resolution
	5 / 3840x2160@60
	3 / 3840x2160@60
	3 / 4096x2160@60
	3 / 4096x2160@60
	4 / 4096x2160@60

	Video outputs
	2 x DisplayPort, 1 x USB-C (DP Alt)
	3 x DisplayPort
	3 x DisplayPort
	2 x HDMI, 1 x USB-C (DP Alt)
	1 x DisplayPort, 1 x HDMI

	USB
	3 x USB 2.0, 1 x USB 3.x, 2 x USB-C
	2 x USB 2.0, 4 x USB 3.x, 1 x USB-C
	4 x USB 2.0, 2 x USB 3.x, 2 x USB-C
	2 x USB 2.0, 2 x USB 3.x, 1 x USB-C
	3 x USB 2.0, 3 x USB 3.x, 1 x USB-C

	Network
	1 GbE, Wi-Fi 7
	1 GbE, Wi-Fi 6
	1 GbE, Wi-Fi 6E
	1 GbE, Wi-Fi 6
	1 GbE, Wi-Fi 7

	VDI platforms
	Citrix, Omnissa Horizon, Azure Virtual Desktop, Windows 365, Microsoft RDS, Amazon WorkSpaces, HP Anyware, Parallels RAS, Frame, Workspot, Leostream
	Citrix, Omnissa Horizon, Microsoft RDS, Azure Virtual Desktop, Windows 365, Amazon WorkSpaces, HP Anyware, Parallels RAS, Frame, Workspot, Leostream
	Citrix, Omnissa Horizon, Microsoft RDS, Azure Virtual Desktop, Parallels RAS, Windows 365, Amazon WorkSpaces, HP Anyware, Frame, Workspot, Leostream
	Citrix, Omnissa Horizon, Azure Virtual Desktop, Windows 365, Microsoft RDS, Amazon WorkSpaces, HP Anyware, Parallels RAS, Frame, Workspot, Leostream
	Citrix, Omnissa Horizon, Azure Virtual Desktop, Windows 365, Amazon WorkSpaces, Microsoft RDS, HP Anyware, Parallels RAS, Frame, Workspot, Leostream

	Optimised UC
	Microsoft Teams, Zoom, Cisco Webex, Cisco Jabber, Skype for Business
	Microsoft Teams, Zoom, Cisco Webex, Cisco Jabber, Skype for Business
	Microsoft Teams, Zoom, Cisco Webex
	Microsoft Teams, Zoom, Cisco Webex, Cisco Jabber
	Microsoft Teams, Zoom, Cisco Webex, Cisco Jabber, Skype for Business

	Management
	Wyse Management Suite
	HP Wolf Cloud Endpoint Manager (HP Cloud Endpoint Manager); HP Device Manager
	ThinMan
	10ZiG Manager
	IGEL management (IGEL Cloud Gateway) when ordered with IGEL OS



9. Assumptions and sources
· Specifications were read from each OEM's own website; options vary by region and change with OS and firmware releases.
· A value an OEM does not publish is shown as "to confirm" and scored low - it is never assumed to be supported.
· Platform or Teams support marked "via OS" is what the operating system's vendor lists; "inferred" means Windows IoT Enterprise runs the Windows client and the OEM does not state it itself.
· The per-seat CPU and memory baseline and the bandwidth figures are planning rules of thumb, not OEM figures - validate them in a pilot.
· USB and printer redirection, and optimised Teams, Zoom or Webex, also depend on the VDI platform version and its policies.
· Licences for the VDI platform, Microsoft 365 and the endpoint operating system are outside the scope of this selection.
Official sources
	Model
	Official product page
	Datasheet

	Dell Pro Micro Thin Client (Q9M1260)
	https://www.dell.com/en-us/shop/wyse-endpoints-and-software/dell-pro-micro-thin-client/spd/dell-pro-q9m1260-thin-client-micro
	https://www.delltechnologies.com/asset/en-us/products/thin-clients/briefs-summaries/dell-pro-micro-thin-client-product-brochure.pdf

	HP Elite t655 Thin Client
	https://h20195.www2.hp.com/v2/GetDocument.aspx?docname=c08327446
	https://h20195.www2.hp.com/v2/GetDocument.aspx?docname=c08623616

	Praim Meridian (M9354 / M9311 / M9321)
	https://www.praim.com/en/solutions/thinclient/meridian/
	https://www.praim.com/wp-content/uploads/2025/04/Meridian-datasheet-Praim-REV.EN-2025-04-01.pdf

	10ZiG 7300q Series (7372q / 7311q)
	https://www.10zig.com/product/solutions/thin-clients/7300q-series/
	https://www.10zig.com/wp-content/uploads/2026/08/7300q-Series-Spec-Sheet-8_28_26.pdf

	Lenovo ThinkCentre M75q Gen 5
	https://psref.lenovo.com/Product/ThinkCentre/ThinkCentre_M75q_Gen_5
	https://psref.lenovo.com/syspool/Sys/PDF/ThinkCentre/ThinkCentre_M75q_Gen_5/ThinkCentre_M75q_Gen_5_Spec.pdf

	LG CQ601 (CQ601N / CQ601I / CQ601W)
	https://www.lg.com/global/business/monitors-pcs/thin-clients/desktop-thin-clients/cq601w/
	https://media.us.lg.com/m/477f7ca62f07dbc6/original/CQ601W-BP-Spec-Sheet.pdf

	Centerm D650
	https://www.centermclient.com/uploads/Centerm-D650-datasheet.pdf
	https://www.centermclient.com/uploads/Centerm-D650-datasheet.pdf

	ZeeTim ZeeTerm ZTX6002
	https://zeetim.com/products/thin-client-zeeterm
	-

	NComputing EX500S
	https://www.ncomputing.com/documentation/datasheet/ex500w-datasheet/249046
	https://ncomputing.box.com/shared/static/f4xx38z27g20z40f6b4z73b71x7alvq3.pdf

	Rangee Thin Client RT-603
	https://rangee.com/en/rangee-thin-client-rt-603/
	https://rangee.com/wp-content/uploads/2026/02/Rangee_Datasheet_RT-603_EN-1.pdf

	ClearCube CD8810
	https://clearcube.com/products/thin-clients/cd8810/
	https://images.clearcube.com/wp-content/uploads/2026/03/04155516/DS-Thin-Client-CD8810.pdf

	Atrust t175W
	https://www.atrustcorp.com/products/t175w/
	https://www.atrustcorp.com/wp-content/uploads/2022/04/t175W-Specification.pdf

	Chip PC iX PC Core Wifi
	https://chippc.com/product/ix-pc-mini-5100-wifi-thinx-os/
	-

	Leadtek EL4115 Ultra-Thin Client
	https://www.leadtek.com/eng/products/virtual_DS(24)/EL4115_Ultra-Thin_Client(40986)/detail
	-

	Fujitsu ESPRIMO G6016-TC
	https://jp.fujitsu.com/platform/pc/product/specific_use/thinclient_model/g6016tc/spec.html
	-

	Amulet Hotkey DX1500
	https://www.amulethotkey.com/product/dx1500/
	https://www.amulethotkey.com/wp-content/uploads/2026/02/DX1500-Datasheet-v1.0.pdf

	OnLogic TM260
	https://www.onlogic.com/store/tm260/
	https://media.onlogic.com/248f8472-1b41-4a43-9f88-4aee598a9ac5/ddd8c62e-1eeb-405c-b13c-699c411b5cee/8GG6HTdcH8XAbyUfOD7BuackD/VJHfXNYmoYIRWxPkHJf44g5bH.pdf

	Clientron G610
	https://www.clientron.com/en/product.php?act=view&id=79
	https://www.clientron.com/data/file/202607/1784518880441507258.pdf

	openthinclient ThinClient BLACK.QUADRO.II
	https://openthinclient.com/en/product-2/nvidia-quadro-2-thin-client/
	-

	Pepperl+Fuchs BTC22
	https://www.pepperl-fuchs.com/en/landingpage/explosion-protection/industrial-box-thin-client-btc-gp27893
	https://files.pepperl-fuchs.com/webcat/navi/productInfo/doct/tdoct9440__eng.pdf?v=19-SEP-24

	epatec Thin Client 13G
	https://www.epatec.de/shop/thin-client-13g-70
	-

	RDP Thin Client C212261
	https://rdp.in/corporate/thin-clients
	-

	Raspberry Pi 500
	https://www.raspberrypi.com/products/raspberry-pi-500/
	https://pip.raspberrypi.com/documents/RP-008349-DS-raspberry-pi-500-product-brief.pdf

	Advantech TPC-312 EHL
	https://www.advantech.com/en-us/products/2f7a6598-a2be-40d6-b615-adb84b164442/tpc-312-ehl/mod_b7f4615d-4c5f-469b-9cbc-1b4a8a27719a
	https://advdownload.advantech.com/productfile/PIS/TPC-312%20EHL/file/TPC-300-EHL_DS(070926)20260714102324.pdf

	Microsoft Windows 365 Link
	https://learn.microsoft.com/en-us/windows-365/link/whats-in-the-box
	-

	Rockwell ASEM 6300T-BB Dual DisplayPort Thin Client
	https://www.rockwellautomation.com/en-us/products/hardware/industrial-computers-monitors/6300t-box-thin-client.html
	https://literature.rockwellautomation.com/idc/groups/literature/documents/td/6300-td001_-en-p.pdf

	IGEL UD Pocket 2
	https://kb.igel.com/en/hardware/current/technical-specification-of-ud-pocket-2
	-

	vCloudPoint V1
	https://www.vcloudpoint.com/zero-clients/zero-client-comparison/
	https://www.vcloudpoint.com/wp-content/uploads/documentations/A1-S100-V1-Datasheet-EN.pdf

	Thinvent Micro 6 Pro
	https://www.thinvent.in/p/P-6P-o4-e64-5_2P-D-Thinux-0
	-



Head office VDI endpoint refresh - Generated by the Niyya Zero/Thin Client Selector - niyyasoft.com	Page 1
implementation.png
Implementation design - Head office VDI endpoint refresh
263 x Dell Pro Micro Thin Client (Q9M1260) - seat wiring, network path, quantities and rollout

SEAT BUILD - REPEATED 250 TIMES
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Managed devices
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Power adapters, rated
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about 255 Mbps

16.3 kW across the seats

@ Power

NETWORK PATH - DESK TO DESKTOP
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Access switch x 6

250 ports at 1 GbE, endpoint VLAN Suite
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Core and firewall
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ROLLOUT
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NetScaler Gateway / Citrix Gateway Service : Direct to the UC
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MANAGEMENT

Wyse Management

HTTPS from every

Microsoft Teams

cloud, not through

° Stand up Wyse Management Suite and enrol one test device (DHCP option

or DNS record for auto-discovery).

o Build the device profile: Dell ThinOS 10.x, Citrix Workspace app,
2-display layout, Microsoft Teams optimisation, peripheral and USB
policy.

Prepare the network: endpoint VLAN and DHCP scope for 263 devices, 1

GbE access ports, QoS for real-time media, firewall rules (TCP/UDP 443
through the gateway; 1494 / 2598 on the LAN).

Pilot 10 seats across the knowledge worker use case; measure session
bandwidth against the 0.9 Mbps per-session estimate.

Roll out by floor or site: 250 seats, zero-touch enrolment, asset
tags, user sign-off per batch.

support contacts.

Ports: Dell Technologies, dell.com

Hand over: 13 spares on the shelf, firmware and OS update cadence, OEM
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Logical design - Head office VDI endpoint refresh
263 x Dell Pro Micro Thin Client (Q9M1260) - Citrix - Citrix HDX (ICA)
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USERS MANAGEMENT
250 knowledge worker seats at Riyadh HQ - Virtual desktops (VDI) - 80% signed in at peak Wyse Management Suite

Profiles, firmware and OS updates,
asset inventory and remote shadowing
for every endpoint.

ENDPOINT - ONE PER SEAT

Dell Pro Micro Thin Client (Q9M1260) At the desk
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Thin client - Desktop box i
. P 2 x Full HD monitors Keyboard + mouse Webcam COLLABORATION
05: Dell ThinOS 10.x d ; Microsoft Teams optimised
Client: Citrix Workspace app Headset Printer
Audio and video are encoded on the
8 cores - 8 GB - 1 GbE endpoint and go straight to the UC
service; only signalling stays in the
session.
Citrix HDX (ICA)
TCP/UDP 443 through the gateway; 1494 / 2598 on the LAN ———————

PERIPHERAL REDIRECTION

NETWORK
Webcam, Headset, Printer
Access switch Campus LAN Firewall USB and printer redirection are
1 GbE to the desk about 255 Mbps at peak only the protocol ports open policies of the VDI platform - allow
l only the device classes listed.

SECURE ACCESS AND BROKERING
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Sessions are encrypted end to end;
multi-factor sign-in is enforced at the
gateway.

DESKTOPS AND APPS - CITRIX

VDAs: virtual desktops and published apps

200 concurrent sessions at peak - delivered as virtual desktops (VDI)

Device specifications: Dell Technologies, dell.com - Dashed lines: management and media paths outside the session Niyya Software - Zero/Thin Client Selector




